Eagle.com

Version 4.01.Copyright (C) Cirrus Logic Inc., 1987-1990.  
All Rights Reserved.

Video BIOS Version 2.20 or later is required to run this utility.

Use Eagle -? for more information on keywords and options.

Usage is: [ -dsvc ]
-d           Gives System ROM BIOS Date
-s           Gives status information
-v           Gives extended status information 
-c           Gives dot clocks in extended status information

Some of the responses:
EGA or CGA (From EGA State).
MGA (From EGA State).
EGA Enhanced Text.
	other: VGA.CGA.MGA.
VGA Enhanced Text: Monochrome, Color, Enhanced Color. 
Digital Multi-Frequency: Unknown type, IBM PS/2 Analog.
Analog Multi-Frequency: Display type is set to .CRT.
Expanded mode is enabled/disabled.
Ram access is set to:
	allow 16 bit.
	force 8 bit.
Reverse video is set to:
	enable reverse video.
	disable reverse video.
Attribute emulation is set to:
	AUTOMAP.

Menu operation: 
Use the UP and DOWN arrow keys to move up and down, 
the [Enter].key to select an item, or the [Esc] to key to exit to DOS.
AUTO: Auto Switch.
COLOR: Select COLOR mode 
Select STANDARD VGA bandwidth: Standard or FAST.
CRT: Switch the display to CRT.
EXPAND: Enable EXPAND mode
REVERSE: Enable REVERSE VIDEO
BOLD: Enable BOLD mode
Enable ATTRIBUTE EMULATION
AUTOMAP: Automap or CENTER
NO16BIT: Force 8 bit operation
EXIT: Exit to DOS
VGA Color State: VGA Mono State, CGA State, MGA State, Hercules Half Mode, Hercules Full Mode.
REBOOT: Reboot System in Current State. 
LOCK: Lock the Current State. [ LOCK ].
VIDEO MODE SWITCH UTILITY: Switch the display to CRT 
Switch to 132 x 25 Mode
Switch to 132 x 43 Mode
Switch to 800 x 600 Mode
Set 200 Scan Line Text Modes
Set 350 Scan Line Text Modes
Set 400 Scan Line Text Modes


