11-03-95

		GDS7543 DOS Utilities & Driver  2.10
		-------------------------------------
	                GD7543 rev BC/BF silicon


Changes from release 2.00 to 2.10
=================================

-CLMODE.EXE has been updated to better support TV options in Panel Control
 menu.

-CLMODE.EXE fixed some foreign languages characters corruption problems.

-No change in AutoCAD driver.


INSTALLATION
============

1. Insert DOS driver diskette in drive a: or b:.
2. Change to drive a: or b:.
3. Type EINSTALL [Enter] from a:\ or b:\.
4. Follow instruction on screen.


UTILITIES NOTES
===============

CLMODE.EXE is not designed to run in Windows Virtual DOS mode.


TurboDLDclassic Driver
======================

-AutoShade 386 rendering is not supported.

-Switcher.com does not support display type switching ( panel-> CRT, etc.) 
 while running any resolution other than VGA.  If user wants to change display
 type, exit the current AutoDesk application and then change display type 
 with either SWITCHER.COM or CLMODE.EXE.


Testing Anomalies
=================

The following items were discovered during testing against the test plan 
documented in the release notes:


-CLMODE.EXE caused an "exception 13: conflicts between two applications"
 error message with QEMM v7.01, 7.02.  This is determined to be a 
 QEMM deficiency.  Earlier version and later version of QEMM solved this
 problem.




